## Stringers installer for a custom staircase

In Mirabel, Saint-Sauveur, Saint-Donat and throughout the Laurentians, Rampe et Moustiquaire offers sales and professional installation services for custom aluminum staircases. As an authorized distributor and installer of aluminum stair stringers from the manufacturer Déco-Rampe, we are able to offer you the aluminum stair stringers as well as the fibreglass or aluminum stair treads you need.

All our stair stringers and other stair components are covered by a 20-year transferable limited warranty offered by the manufacturer.

## Stringers for staircases

Whether it is for your home, your business, your institutional building or your industrial building, you can choose the model of aluminum staircase that will best meet your aesthetic needs: staircase with open aluminum stringers, staircase with closed aluminum stringers or staircase with Heritage aluminum stringers.

To complete your custom aluminum staircase, we sell and install aluminum stair treads and fibreglass stair treads. Different models of aluminum handrails, posts and balusters will be offered to give a unique look to your staircase, and you will be presented a range of colours for greater personalization.

## Stair stringer installer

Your exterior aluminum staircase must be designed and installed in accordance with the standards of the Régie du bâtiment du Québec to be safe and durable. Our installation services for stairs with aluminum stair stringers (and aluminum or fibreglass steps) are offered in residential, commercial, institutional and industrial environments. Our team can build staircases that meet your specific needs: height, size of steps, material used, colour, etc.

The dimensions of the stairs are regulated, and the installation methods used to install stair stringers must comply fully with all Construction Code standards. Whether it is a balcony staircase, a corner staircase or a staircase located on the second floor of a building, our rigorous installation methods ensure your total safety.

The spacing between each stair stringer must not exceed 42 inches. A wider space would put too much weight on the steps and create micro cracks in the fibreglass. For stairs wider than 42 inches, it is mandatory to add a third stringboard in the middle to ensure that the weight is well distributed and that the staircase supports the people using it.

## Contact us

For the purchase and installation of a custom aluminum staircase as well as for safe and professional installation of your staircase, contact us at 514-261-1384. You can also request a free assessment and a free quote!

The Rampe et Moustiquaire team travels to Mirabel, Saint-Sauveur, Saint-Donat and to all other cities in the Laurentians region for an installation of custom aluminum staircases.